In project:

* Car (40cm x 18cm).
* Street (2 lines- the width: 60cm).
* The speed of Car (40 km/h).

In reality:

* According to Toyota Camry lengthx widthx height: 4825x 1820x 1480 (mm)

<http://i-view.vn/i-view-news/44-tinchuyenganhkientrucnoithat/57-kich-thuoc-xe-oto-thong-dung>

* According to table 3- Technical table decentralized functional motorways of the road and design flow and table 6- Minimum width elements on the cross for plain and hilly terrain.
* Car will run on a street which is at IV level.
* The speed of car is about 60 km/h.
* The width of a line in a street (2 lines): 3.5m.

<http://cucqlxd.gov.vn/media/documents/tcvn_4054_2005.pdf>

Both the project and reality, the car run on a street which has a lot of obtacles such as human, other cars, motorbike, bike and across corners.

